|  |  |
| --- | --- |
| **HARDWARE FEATURES** | |
| Standards and Protocols | IEEE 802.3i, IEEE 802.3u, IEEE 802.3x |
| Interface | 24 10/100Mbps RJ45 Ports (Auto Negotiation/Auto MDI/MDIX) |
| Network Media | 10BASE-T: UTP category 3, 4, 5 cable (maximum 100m) 100BASE-TX: UTP category 5, 5e or above cable (maximum 100m) |
| Fan Quantity | Fanless |
| Physical Security Lock | Yes |
| Power Supply | 100-240VAC, 50/60Hz 0.6A |
| Dimensions ( W x D x H ) | 17.3\*7.1\*1.7 in. (440\*180\*44 mm) |
| Mounting | Rack Mountable |
| Max Power Consumption | 3.19W(220V/50Hz) |
| Max Heat Dissipation | 10.88BTU/h |
| **PERFORMANCE** | |
| Switching Capacity | 4.8Gbps |
| Packet Forwarding Rate | 3.57Mpps |
| MAC Address Table | 8K |
| Buffer Memory | 2Mb |
| Advanced Functions | Green Technology 802.3X Flow Control |
| Green Technology | Innovative energy-efficient technology saves power up to 75% |
| Transfer Method | Store-and-Forward |
| **OTHERS** | |
| Certification | FCC, CE, RoHS |
| Package Contents | 24-Port 10/100Mbps Fast Ethernet Switch Power Cord Installation Guide Rackmount Kit Rubber Feet |